

|  |  |  |
| --- | --- | --- |
| **SAP Data Entry for Extensions**  **Please complete as fully as possible and email to jerry@c2cdartmouth.co.uk**  **Please note that construction drawings including plan, elevation and sectional views will be required along with a schedule of window, door and roof light specifications, dimensions and locations.**  **PDF or CAD plans are preferred. Paper versions may be accommodated at additional cost but please note that photocopies cannot be used as the scale may be distorted.**  Contact Name | | |
| Contact Email | | |
| Contact Number | | |
| Property Name | | |
| Property Address | | |
| Property Type (House, bungalow etc.) | | |
| Property Type (End Terrace, detached etc.) | | |
| Property Orientation (where does the front door face?)(NSEW)  Existing Property Date Built | | |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
| **New Extension Wall Construction (from external to internal)**  e.g. mm brickwork, mm cavity, mm polystyrene, mm Thermalite turbo block, mm plaster      U-Value (W/m²K) achieved if known | |
| **New Extension Secondary Wall Construction (from external to internal)**  e.g. mm brickwork, mm cavity, mm polystyrene, mm Thermalite turbo block, mm plaster  Please include details of internal partitions and room in roof stud walls.      U-Value (W/m²K) achieved if known | |
| **New Extension Roof Construction (external to internal)**  E.g. Pitched roof with insulation at rafters, pitched roof insulated flat ceiling or flat roof.  Please give full details of all layers. | |
| U-Value (W/m²K) achieved if known | |
|  | |
| **New Extension Ground Floor Details (external to internal)**  e.g. mm Concrete Slab, mm Kingspan K103, mm screed etc | |
| U-Value (W/m²K) achieved if known | |
| **New Extension Glazing Type**  Single Glazing Double Glazing Triple Glazing    Double/Triple Glazing Air Gap 6mm 12mm 16mm 20mm 24mm Other | |
| New Extension Window Frame Type(upvc/aluminium/timber/composite)  **Window Properties**  K Glass  Argon Filled  Soft Coat  Hard Coat  Low e | |
| Window U-Value (W/m²K) if known, for whole frame unit from manufacturer’s specification    Door U-Value (W/m²K) if known, for whole frame unit from manufacturer’s specification (note doors with over 60% glazing are treated as windows e.g. patio doors) | |
| Total area of openings removed as part of project | |
|  | |
|  | |
|  | |
|  | |
| |  | | --- | | Additional Information: | | |

**I certify that these details are correct to the best of my knowledge.**

|  |
| --- |
| Signed  Name (Print) |

|  |
| --- |
| Position  Date |