

|  |
| --- |
| **SAP Data Entry for Extensions** **Please complete as fully as possible and email to jerry@c2cdartmouth.co.uk** **Please note that construction drawings including plan, elevation and sectional views will be required along with a schedule of window, door and roof light specifications, dimensions and locations.****PDF or CAD plans are preferred. Paper versions may be accommodated at additional cost but please note that photocopies cannot be used as the scale may be distorted.**Contact Name  |
| Contact Email  |
| Contact Number  |
| Property Name  |
| Property Address  |
| Property Type (House, bungalow etc.)  |
| Property Type (End Terrace, detached etc.)  |
| Property Orientation (where does the front door face?)(NSEW)  Existing Property Date Built   |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
| **New Extension Wall Construction (from external to internal)**e.g. mm brickwork, mm cavity, mm polystyrene, mm Thermalite turbo block, mm plaster  U-Value (W/m²K) achieved if known |
| **New Extension Secondary Wall Construction (from external to internal)**e.g. mm brickwork, mm cavity, mm polystyrene, mm Thermalite turbo block, mm plasterPlease include details of internal partitions and room in roof stud walls.  U-Value (W/m²K) achieved if known |
| **New Extension Roof Construction (external to internal)**E.g. Pitched roof with insulation at rafters, pitched roof insulated flat ceiling or flat roof.Please give full details of all layers. |
| U-Value (W/m²K) achieved if known |
|  |
| **New Extension Ground Floor Details (external to internal)**e.g. mm Concrete Slab, mm Kingspan K103, mm screed etc  |
| U-Value (W/m²K) achieved if known |
| **New Extension Glazing Type** Single Glazing Double Glazing Triple Glazing  Double/Triple Glazing Air Gap 6mm 12mm 16mm 20mm 24mm Other |
| New Extension Window Frame Type(upvc/aluminium/timber/composite) **Window Properties** K Glass  Argon Filled  Soft Coat  Hard Coat  Low e |
| Window U-Value (W/m²K) if known, for whole frame unit from manufacturer’s specificationDoor U-Value (W/m²K) if known, for whole frame unit from manufacturer’s specification (note doors with over 60% glazing are treated as windows e.g. patio doors) |
| Total area of openings removed as part of project |
|  |
|  |
|  |
|  |
|

|  |
| --- |
| Additional Information: |

 |

**I certify that these details are correct to the best of my knowledge.**

|  |
| --- |
| Signed  Name (Print)  |

|  |
| --- |
| Position  Date  |